**20W-50 SG/CD LPG**

20W-50 LPG, is an engine oil that is produced especially for cars and light commercial vehicles working with LPG and can be used safely in all seasons. It is produced by adding specially developed performance additives to high quality mineral-based base oils. It is especially recom- mended for passenger vehicles that operate under difficult conditions and frequently stop and go.

**Certificates And Standards:**

API SJ/CD,

ACEA A3/B3-04,

MB 228.3, 229.1

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Appearance** | Visual | Clear-Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 16,3-21,9 |
| **Viscosity Index** | ASTM D2270 | Min. 110 |
| **Flash Point, °C** | ASTM D92 | Min. 200 |
| **Pour Point, °C** | ASTM D97 | Max. -21 |
|  |  |  |