**5W-30 SN/CF**

Is four season engine oil which has been formulated with synthetic oils and performance additives for superior protection and excellent fluidity. It has been developed to be used in diesel engines Passenger and commercial vehicles engines which work by gasoline. It can be safely used in Cars, vans and small commercial vehicles engines.

**Certificates And Standards:**

API SN, API SM, API SL, API CF,

ACEA C2-10, ACEA C2 / C3,

 MB-Approval 229.51,

VW 504.00, VW 507.00,

GM DEXOS 2

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Appearance** | Visual | Clear-Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 9,3 - 12,5 |
| **Viscosity Index** | ASTM D2270 | Min. 155 |
| **Flash Point, °C** | ASTM D92 | Min. 200 |
| **Pour Point, °C** | ASTM D97 | Max. -36 |
|  |  |  |