**5W-40 SN/CF**

5W-40 is full synthetic engine oil which perfectly adapted to all types of modern vehicles, passenger cars, SUVs and off-road cars equipped and using unleaded fuel or liquefied petroleum gas (LPG). It is particularly suited to turbocharged, multi-valve and direct injection engines.

**Certificates and Standards:**

API SN, API SM, API SL, API CF,

MB-Approval 226.5, MB-Approval 229.31, MB-Approval 229.51,

VW 502.00, VW 505.00, VW 505.01

RENAULT RN 0710/0700

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Appearance** | Visual | Clear-Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 12,5-16,3 |
| **Viscosity Index** | ASTM D2270 | Min. 150 |
| **Flash Point, °C** | ASTM D92 | Min. 220 |
| **Pour Point, °C** | ASTM D97 | Max. -35 |
|  |  |  |