**10W-30 CI-4/SL**

10W/30 is a synthetic engine oil that is prepared by synthetic base oils and advanced technology performance additive packages. Its usage is recommended for passenger cars and commercial vehicles, European and American design, low-emission, turbocharged engines. It is also recommended for vehicles that are working on roads and high speed / heavy load, light and heavy truck transport over short distances as well as upload / download operating, construction and agricultural land, such as vehicles running under heavy load conditions.

**Certificates And Standards:**

API CI-4/SL,

Renault RVI RXD,

Volvo VDS -2 / VDS - 3,

MB 228,5

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 9,3-12,5 |
| **Viscosity Index** | ASTM D2270 | Min. 130 |
| **Flash Point, °C** | ASTM D92 | Min. 220 |
| **Pour Point, °C** | ASTM D97 | Max. -30 |