**15W-40 SHPD CI-4/SL**

15W/40, Is super high performance (SHPD) diesel engine oil which has been developed for use in next-generation heavy duty diesel engines can be safely used four seasons. It is formulated with high quality base oils by adding superior performance additives. It is recommended for use in heavy duty vehicles and construction equipment of diesel engines with or without turbocharger.

**Certificates And Standards:**

API CI-4/CH-4/SL ACEA E7/E5/E3/E2, MB 228.3, MAN M3275, Mack EO – M PLUS, MTU Type 2, Volvo VDS-3 /VDS-2, Renault RLD/RLD-2, Cummins 20078 / 20077 / 20076, CAT ECF -2

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 12,5-16,3 |
| **Viscosity Index** | ASTM D2270 | Min. 130 |
| **Flash Point, °C** | ASTM D92 | Min. 220 |
| **Pour Point, °C** | ASTM D97 | Max. -27 |