**5W-30 CI-4/SL**

5W/30, is a synthetic engine oil developed with superior additive formulation for passenger cars and light diesel vehicles. It meets all the requirements of diesel engines produced with modern technology. It shows unmatched performance in all four seasons. With its high viscosity index, it provides a unique protection for the engine in all climate and road conditions.

**Certificates And Standards:**

API CI-4/SL,

Renault RVI RXD,

Volvo VDS-2/VDS-3,

MB 228.5

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 9,3-12,5 |
| **Viscosity Index** | ASTM D2270 | Min. 130 |
| **Flash Point, °C** | ASTM D92 | Min. 220 |
| **Pour Point, °C** | ASTM D97 | Max. -35 |