**H SERIES CA/SA**

 Is monograde, economic oils containing high quality additives, developed for medium load, normal speed diesel and gasoline engines. It makes effective lubrication, prevents wear, extends the life of the engine.

**Certificates And Standards:**

API CA/SA

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
|  |  **10 30**  |  **30 40 50 60** |
| **Appearance** | Visual |  Clear & Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 4,5-6,5  |  9,3-12,5 12,5-16,3 16,3-21,9 21,9-26,1  |
| **Viscosity Index** | ASTM D2270 min. 100 |  min. 90 min.90 min.90 min.90  |
| **Flash Point, °C** | ASTM D92 min. 185 |  min. 220 min.220 min.220 min.220  |
| **Pour Point, °C** | ASTM D97 max. -24 | max. -15 max.-15 max.-15 max.-10  |
|  |  |  |