**HDX SERIES CF/SF**

Is engine oil that is prepared by using base oils obtained through modern refining processes and qualified additives, and that is intended to be used in diesel vehicles operating under heavy conditions. It keeps engine clean under any kind of climate and road condition. It provides protection against abrasion, corrosion and oxidation.

**Certificates And Standards:**

API CF/SF

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
|  | **10 30** | **30 40 50 60** |
| **Appearance** | Visual | Clear & Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 4,5-6,5 | 9,3-12,5 12,5-16,3 16,3-21,9 21,9-26,1 |
| **Viscosity Index** | ASTM D2270 min. 100 | min. 90 min.90 min.90 min.90 |
| **Flash Point, °C** | ASTM D92 min. 185 | min. 220 min.220 min.220 min.220 |
| **Pour Point, °C** | ASTM D97 max. -27 | max. -15 max.-15 max.-15 max.-10 |
|  |  |  |