**HYDRAULIC OIL 32**

HYDRAULIC OIL, is high quality hydraulic oils which formulated with quality base oils and oxidation, corrosion and rust inhibitors additives. It is recommended to use in many industrial and mobile hydraulic systems.

 **Certificates And Standards:**

|  |  |  |
| --- | --- | --- |
| DIN 51524 Part 2, Denison HF-0, HF-1, HF-2, Cincinnati Machine P-68, P-69, P-70, U.S. Steel 127, U.S. Steel 136, Bosch Rexroth, Eaton Vickers M-2950-S, AFNOR NFE 48-690, NFE 48-691, Eaton Vickers I-286-S, GM LS-2, JCMAS HK, SAE MS1004 |  |  |

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (40°C), [cSt]** |  ASTM D445 |  28,8-35,20 |
| **Viscosity Index** |  ASTM D2270 | Min. 100 |
| **Flash Point, °C** | ASTM D92 | Min. 205 |
| **Pour Point, °C** | ASTM D97 | Max. -25 |