**ECOBENNZ 4T 20W/50**

4T 20W-50 combine highly refined quality mineral oils and advanced additives to provide good engine cleanliness, good wear protection and corrosion protection. It’s suitable all seasons for air cooled/liquid-cooled 4-stroke engines and wet clutches.

|  |  |  |  |
| --- | --- | --- | --- |
| **Certificates And Standards:**  API SL, JASO MA (T903:2011), JASO MA2 (T903:2011) |  |  |  |

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 16,3-21,9 |
| **Viscosity Index** | ASTM D2270 | Min. 115 |
| **Flash Point, °C** | ASTM D92 | Min. 220 |
| **Pour Point, °C** | ASTM D97 | Max. -21 |