**SAE 90 GL-4**

90W, is special gear oil which is formulated with superior additives and mineral base oils derived from modern refining. It’s manual transmission fluid for mechanical gearboxes and axles in cars and trucks as well as construction and agricultural machinery.

**Certificates And Standards:**

|  |  |  |
| --- | --- | --- |
| API GL-4, David Brown S1.53.101(E), U.S. Steel 224, DIN 51517 Part 3, AGMA 9005-D94ZF TE-ML 02A, 08, 16A, 17A, 19A |  |  |

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 |  13,5-18,5 |
| **Viscosity Index** | ASTM D2270 | Min. 92 |
| **Flash Point, °C** | ASTM D92 | Min. 225 |
| **Pour Point, °C** | ASTM D97 | Max. -18 |