**20W-50 SL/CF**

It is a gasoline engine oil produced by blending high quality base oils with high performance additives. Engine oil that can be use by confidence for four seasons especially heavily used gasoline and LPG vehicles in urban traffic.

**Certificates And Standards:**

API SL/CF

VW 501.01 / 505.00

ACEA A3/B4

MB Approval 229.1

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Appearance** | Visual | Clear-Bright |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 16,3-21,9 |
| **Viscosity Index** | ASTM D2270 | Min. 110 |
| **Flash Point, °C** | ASTM D92 | Min. 200 |
| **Pour Point, °C** | ASTM D97 | Max. -21 |
|  |  |  |