**0W-40 SN/CF**

0W40, An advanced synthetic engine oil designed to help provide excellent engine cleaning power, wear protection and overall performance.

**Certificates And Standards:**

API SN, API SM, API SL, API CF,

ACEA A3/B4, ACEA A3/B3,

AAE (STO 0003) GROUP B7

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Kinematic Viscosity (100°C), [cSt]** | ASTM D445 | 12,5-16,3 |
| **Viscosity Index** | ASTM D2270 | Min. 150 |
| **Flash Point, °C** | ASTM D92 | Min. 225 |
| **Pour Point, °C** | ASTM D97 | Max. -39 |